**YOUTH MIDSIZE FWD RULES**

**These rules are plain and simple, cut and dry!!! What is said below is exactly what you can do and nothing else. Don’t try and do anything else cause most likely you will just be loaded!**

Car must be stripped of all internals and outside plastic as well as all windows. Dash may stay in the car.

NO CARB CONVERSIONS! Motor must be from factory to that car. No swapping. Harnesses are ok to use.

Steering, peddles, shifter are ok to use to make things easier for kids

Roof Sign Required

Body shaping is ok. Prerans ok if they fit the rules **(FWD CARS ONLY) 4 or 6 cyl cars only! 110 wheelbase and under!**

Header ok to use.

**CAGE**

Full 4 point cage must be welded or bolted in car for safety of driver and passenger. Cars with anything less will not run. 6x6 material no bigger. Tank can be mounted to back of cage bar or bolted through floor. IF IN FRONT OF REAR AXLE CAN BE LEFT UNDER CAR.

2 front windshield bars must be added. 9 wire, 2x2 straps, chain

**DOORS, HOOD, TRUNK**

Drivers door may be welded shut Also may be skinned for safety. Other seams get 2 3x3 1/8 inch plate per seam.

Hood and Trunk must have 12x12 hole in them.

No duck tape on doors

**BUMPERS**

**Factory car bumper may be used and may be stuffed inside only or a 3x3 square tube. These are your 2 options**

**You may use a 5 inch piece of 3x3 to mount bumper so bumper does not fall off. Nothing else.**

**TIRES**

May run any tire on the front. donuts or forklifts on rear.